Directions:
Paste the files in this folder into the data folder in your desired car. 
(if you're using Content Manager, enable developer mode so you can unpack the data.acd. That way it creates a data folder if it doesn't have one already. Make sure to backup your stock data.acd (rename it from data.acd to databackup.acd) before doing this.)


You need to edit only 2 files:

-kers_torque.lut

-ers1_speed.lut


KERS_Torque.lut: 2 Step Engagement Point. Set the middle RPM to whatever you decide. The bottom and top RPM's will ALWAYS have a 0 value unless the 2 step cuts off because the power of the car overpowers the 2 step.
The middle RPM should always have a higher torque value than the car (300+Nm over the car is recommended)

For example: Camaro ZL1, 650bhp, 881Nm/650Lbft

RPM|Torque
4400|0         top rpm
4500|-1200     middle rpm (engagement point in Nm)
4600|0         bottom rpm

or if it cuts off:
RPM|Torque
4400|0     
4500|-1200    
4600|-1200
5000|-1200
apply a negative torque value at higher rpm's to avoid a cut off        


ERS1_speed.lut: 2 Step Shut Off Point (by speed). The left value will be your speed in Km/h. The right value will be set to either a 1 value, meaning the 2 step limiter will still be active at that speed, or a 0 value, signaling a shut off.

For example:

speed(km/h)|activation #
5|1 (activated)
6|0 (shut off)

YOU DO NOT NEED TO MAP KERS ACTIVATION BUTTON FOR LAUNCH CONTROL